Orange -AN1

White with Black stripes -AN2

Brown -IN1

White -IN2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Signal | Teensy Pin | Color | J8 PORT | Resistors |
| AN1 | 5 | Orange | 5 | 10K to ground |
| AN2 | 6 | White with Black Stripes | 6 | 10K to ground |
| IN1 | 4 | Brown | 1 | 10K to ground |
| IN2 | 7 | White | 2 | 10K to ground |

USB C power supply is connected to 5V power adapter.

4